Install this if you want to use the E28 module on a Windows XP machine.  You must have SP3 installed on your XP machine.  Unzip the files, and run the driver installation tool exe file.  This driver will not work with versions of Windows earlier then XP.  This driver may also be used with Windows 7 and Windows 8 if needed.  Both 32-bit and 64-bit drivers are included.  Find the sub-folder to suit your system from within the ZIP file, and run the driver installation tool.  This will tell you it is installing a 2200 series driver, but this also works with the 1455 chip used as the USB interface on the E28 module.

Windows 10 has native support for this USB chip, so no driver files are needed.  Windows 7 and 8 should also pick up on this chip without the driver, but on some systems that have not had automatic updates turned on, you might still need to install this driver under those systems.

Linux should pick up on this device without drivers, and assign it to the tree under /dev/ttyACM0.   


G.
15/12/2017